Safety Data Sheet
    SDS Number: 20100
     Issue Date: 06/01/15
    Reviewed: 02-01-22
    	
SECTION 1	PRODUCT IDENTIFICATION	

GHS product Identifier:               Chemlube Premium Hydraulic AW 100 
Synonyms:                              Hydraulic Oil

MANUFACTURER/ ADDRESS:    Chemlube International LLC 
                                                        500 Mamaroneck Ave. 
                                                        Harrison, N.Y. 10528 USA

CHEMTREC –                                (800) 424-9300 
General Assistance Number:      (914) 381 5800 

SECTION 2	HAZARDS IDENTIFICATION 	
OSHA/HCS status:                While this material is not considered hazardous by the OSHA Hazard Communication
                                                     Standard (29 CFR 1910.1200), this SDS contains valuable information critical to the
                                                     safe handling and proper use of the product. This SDS should be retained and available
                                                     for employees and other users of this product.

Classification of the              Not classified.
substance or mixture:

GHS label elements
Signal Word :                         No signal word.
Hazard statements :              No known significant effects or critical hazards.

Precautionary statements
General :                                Avoid contact with eyes, skin and clothing. May be harmful if swallowed. IF IN EYES:
                                                     Rinse cautiously with water for several minutes. If swallowed, do not induce vomiting.
                                                     After handling, always wash hands thoroughly with soap and water. If you feel unwell,
                                                     seek medical attention and show the label when possible. Keep out of reach of children.

Prevention :                           Not applicable.
Response :                             Not applicable.
Storage :                                 Store in a dry place and/or in closed container. Store in accordance with all local,
                                                regional, national and international regulations.
Disposal :                               Dispose of contents and container in accordance with all local, regional, national and
                                                      international regulations.

Hazards not otherwise          None known
classified
SECTION 3	Composition/Information on Ingredients 	

Components	CAS Number	Amount	
Highly refined mineral oil	Mixture	95 – 99 %weight	
Petroleum Additives	Mixture	0.50-1.0 %weight	

Any concentration shown as a range is to protect confidentiality or is due to process variation.

There are no ingredients present which, within the current knowledge of the supplier and in the concentrations
applicable, are classified as hazardous to health or the environment and hence require reporting in this section.
Occupational exposure limits, if available, are listed in Section 8.

SECTION 4	FIRST AID MEASURES	

Description of necessary first aid measures

Eye contact:                   Immediately flush eyes with plenty of water, occasionally lifting the upper and lower
                                         eyelids. Check for and remove any contact lenses. Get medical attention if irritation
                                         occurs.

                                        Flush contaminated skin with plenty of water. Remove contaminated clothing and
                                        shoes. Get medical attention if symptoms occur.
 Inhalation:                     Remove victim to fresh air and keep at rest in a position comfortable for breathing. Get
                                        medical attention if symptoms occur
  
Skin contact:                 Flush contaminated skin with plenty of water. Remove contaminated clothing and shoes.
                                        Get medical attention if symptoms occur.

Ingestion:                       Wash out mouth with water. Remove victim to fresh air and keep at rest in a position
                                        comfortable for breathing. Do not induce vomiting unless directed to do so by medical
                                        personnel. Get medical attention if symptoms occur.

Most important symptoms/effects, acute

Potential acute health effects
Inhalation :         No known significant effects or critical hazards.
Ingestion :          No known significant effects or critical hazards.
Skin contact :     No known significant effects or critical hazards.
Eye contact :      No known significant effects or critical hazards.

Over-exposure signs/symptoms
Inhalation:          No specific data
Ingestion:           No specific data 
Skin contact:      No specific data
Eye contact :      No specific data.

Indication of immediate medical attention and special treatment needed, if necessary
Notes to physician :              Treat symptomatically. Contact poison treatment specialist immediately if large
                                                  quantities have been ingested or inhaled.
Specific treatments :            Treat symptomatically and supportively.
Protection of first-aiders :    No action shall be taken involving any personal risk or without suitable training.

See toxicological information (Section 13)

SECTION 5	FIRE FIGHTING MEASURES	

Specific hazards arising:          In a fire or if heated, a pressure increase will occur and the container may burst.
from the chemical

Extinguishing media
Suitable extinguishing              Use an extinguishing agent suitable for the surrounding fire
Unsuitable extinguishing          None known
media

SECTION 5	FIRE FIGHTING MEASURES	

 Hazardous thermal                     Decomposition products may include the following materials:
 decomposition products            carbon dioxide
                                                       carbon monoxide
                                                       sulfur oxides
                                                       phosphorus oxides
                                                       metal oxide/oxides

Special protective actions:         Promptly isolate the scene by removing all persons from the vicinity of the incident if
 for fire-fighters                            there is a fire. No action shall be taken involving any personal risk or without suitable
                                                       training.

Special protective                       Fire-fighters should wear appropriate protective equipment and self-contained breathing                                                                          
equipment for fire-fighters         apparatus (SCBA) with a full face-piece operated in positive pressure mode
                                                 
SECTION 6	ACCIDENTAL RELEASE MEASURES	
Personal precautions, protective equipment and emergency procedures

For non-emergency                    No action shall be taken involving any personal risk or without suitable training. 
personnel                                     Evacuate surrounding areas. Keep unnecessary and unprotected personnel from
                                                      entering. Do not touch or walk through spilled material. Put on appropriate personal  
                                                      protective equipment
                                        
For emergency responders:       If specialized clothing is required to deal with the spillage, take note of any                 
                                                      in Section 8 on suitable and unsuitable materials. See also the information in "For                  
                                                      non-emergency personnel”.

Environmental precautions:      Avoid dispersal of spilled material and runoff and contact with soil, waterways,drains    
                                                      and sewers. Inform the relevant authorities if the product has caused environmental
                                                      pollution (sewers, waterways, soil or air).

Methods and materials for containment and cleaning up:

   Small spill:                               Stop leak if without risk. Move containers from spill area. Dilute with water and mop up
                                                      if water-soluble. Alternatively, or if water-insoluble, absorb with an inert dry material and
                                                      place in an appropriate waste disposal container. Dispose of via a licensed waste
                                                      disposal contractor.
 
  Large spill:                                Stop leak if without risk. Move containers from spill area. Prevent entry into sewers,
                                                     water courses, basements or confined areas. Wash spillages into an effluent treatment
                                                     plant or proceed as follows. Contain and collect spillage with non-combustible,
                                                     absorbent material e.g. sand, earth, vermiculite or diatomaceous earth and place in
                                                     container for disposal according to local regulations (see Section 13). Dispose of via a
                                                     licensed waste disposal contractor. Note: see Section 1 for emergency contact
                                                     information and Section 13 for waste disposal

SECTION 7	HANDLING AND STORAGE	
Precautions for safe handling:
   Protective measures               Put on appropriate personal protective equipment (see Section 8).
   Advice on general                   Eating, drinking and smoking should be prohibited in areas where this material is   
   occupational hygiene             handled, stored and processed. Workers should wash hands and face before eating,
                                                     drinking and smoking. Remove contaminated clothing and protective equipment before
                                                     entering eating areas. See also Section 8 for additional information on hygiene
                                                     measures.

Conditions for safe storage,     Store in accordance with local regulations. Store in original container protected from
including any                             direct sunlight in a dry, cool and well-ventilated area, away from incompatible materials
incompatibilities                        (see Section 10) and food and drink. Keep container tightly closed and sealed until
                                                     ready for use. Containers that have been opened must be carefully resealed and kept
                                                     upright to prevent leakage. Do not store in unlabeled containers. Use appropriate 
                                                     containment to avoid environmental contamination. 

SECTION 7	HANDLING AND STORAGE	
                                                Bulk Storage Conditions: Maintain all storage tanks in accordance with applicable
                                                regulations. Use necessary controls to monitor tank inventories. Inspect all storage
                                                tanks on a periodic basis. Test tanks and associated piping for tightness. Maintain the
                                                automatic leak detection devices to assure proper working condition.

SECTION 8	EXPOSURE CONTROLS/PERSONAL PROTECTION	
Control parameters
   Occupational exposure limits
      None identified.

Appropriate engineering:     Good general ventilation should be sufficient to control worker exposure to airborne
Controls                                 contaminants.
Environmental exposure      Emissions from ventilation or work process equipment should be checked to ensure
 controls:                                they comply with the requirements of environmental protection legislation. In some
                                                cases, vapor controls, filters or engineering modifications to the process equipment will 
                                                be necessary to reduce emissions to acceptable levels.
 
Individual protection measures
  Hygiene measures              Wash hands, forearms and face thoroughly after handling chemical products, before
                                                eating, smoking and using the lavatory and at the end of the working period.
                                                Appropriate techniques should be used to remove potentially contaminated clothing.
                                                Wash contaminated clothing before reusing. Ensure that eyewash stations and safety
                                            showers are close to the workstation location.

 Eye/face protection             Safety glasses equipped with side shields are recommended as minimum protection in
                                               industrial settings. If contact is possible, the following protection should be worn, unless
                                               the assessment indicates a higher degree of protection: Splash goggles. Safety
                                               eyewear complying with an approved standard should be used when a risk assessment
                                               indicates this is necessary to avoid exposure to liquid splashes, mists, gases or dusts.
                                               If inhalation hazards exist, a full-face respirator may be required.
Skin protection                
   Hand protection:               Chemical-resistant gloves complying with an approved standard should be worn at all
                                          times when handling chemical products if a risk assessment indicates this is necessary
   Body protection:               Personal protective equipment for the body should be selected based on the task being
                                               performed and the risks involved and should be approved by a specialist before
                                               handling this product.
   Other skin protection:      Appropriate footwear and any additional skin protection measures should be selected
                                               based on the task being performed and the risks involved and should be approved by a
                                               specialist before handling this product.
   Respiratory protection:    Use a properly fitted, air-purifying or supplied-air respirator complying with an approved
                                               standard if a risk assessment indicates this is necessary. Respirator selection must be
                                               based on known or anticipated exposure levels, the hazards of the product and the safe
                                               working limits of the selected respirator.       
SECTION 9	PHYSICAL AND CHEMICAL PROPERTIES	

Physical State                       Liquid
Color                                      Amber
Flash Point	                  200 Deg C, 392 Deg F (min)
Upper Flammable Limit       Not determined.
Lower Flammable Limit	    Not determined.
Vapor density		    >1 { Air = 1}.
Specific Gravity		    0.86 (15.6 Deg C)
Water Solubility		    Insoluble.				.
Odor			    Mild
Viscosity		    Kinematic (100C) 10.7 cSt –12.1.0 cSt 
Boiling Point		    289 Deg C, 552 Deg F (Initial)
Pour Point Temperature     <-38C

.

SECTION 10	REACTIVITY AND STABILITY	

Reactivity                              Not expected to be Explosive, Self-Reactive, Self-Heating, or an Organic Peroxide
                                               under US GHS Definition(s).
Chemical stability                The product is stable. 
Possibility of hazardous      Under normal conditions of storage and use, hazardous reactions will not occur
reactions:.
Conditions to avoid              No specific data  .
Incompatible materials        No specific data.
Hazardous decomposition  Under normal conditions of storage and use, hazardous decomposition products should 
Products                                not be produced.
 
SECTION 11	TOXICOLOGICAL INFORMATION	
Information on toxicological effects
 Acute toxicity
 Conclusion/Summary       Distillates (petroleum), hydrotreated heavy paraffinic: Mineral oil mists derived from
                                             highly refined oils are reported to have low acute and sub-acute toxicities in animals.
                                             Effects from single and short-term repeated exposures to high concentrations of mineral
                                             oil mists well above applicable workplace exposure levels include lung inflammatory
                                             reaction, lipoid granuloma formation and lipoid pneumonia. In acute and sub-acute
                                             studies involving exposures to lower concentrations of mineral oil mists at or near
                                             current work place exposure levels produced no significant toxicological effects.
                                             Distillates (petroleum), solvent-dewaxed heavy paraffinic: Mineral oil mists derived
                                             from highly refined oils are reported to have low acute and sub-acute toxicities in
                                             animals. Effects from single and short-term repeated exposures to high concentrations
                                             of mineral oil mists well above applicable workplace exposure levels include lung
                                             inflammatory reaction, lipoid granuloma formation and lipoid pneumonia. In acute and
                                             sub-acute studies involving exposures to lower concentrations of mineral oil mists at or
                                             near current work place exposure levels produced no significant toxicological effects.
Irritation/Corrosion
    Skin                                 No additional information
     Eyes                                No additional information
     Respiratory                    No additional information
Sensitization
     Skin                                 No additional information
     Respiratory                     No additional information
Mutagenicity
      Conclusion/Summary  No additional information 
Carcinogenicity
      Conclusion/Summary  No additional information
Teratogenicity
Conclusion/Summary        No additional information 

Information on the likely    Routes of entry anticipated: Dermal.
routes of exposure
Potential acute health effects
   Eye contact                       No known significant effects or critical hazards
   Inhalation                          No known significant effects or critical hazards.
   Ingestion                           No known significant effects or critical hazards.
   Skin contact                      No known significant effects or critical hazards.

Symptoms related to the physical, chemical and toxicological characteristics
   Eye contact                      No known significant effects or critical hazards.
   Inhalation                         No known significant effects or critical hazards.
   Ingestion                          No known significant effects or critical hazards.
   Skin contact                     No known significant effects or critical hazards

Potential chronic health effects
   General                              No known significant effects or critical hazards.
   Carcinogenicity                No known significant effects or critical hazards.
   Mutagenicity                     No known significant effects or critical hazards.
   Teratogenicity                   No known significant effects or critical hazards.
   Developmental effects     No known significant effects or critical hazards.
   Fertility effects                No known significant effects or critical hazards.
SECTION 12	ECOLOGICAL INFORMATION	
Toxicity
Conclusion/Summary       Not available

Persistence and degradability
Conclusion/Summary       Not available.

Bioaccumulative  
Potential                             Not available

Mobility in soil
Soil/water partition
coefficient (KOC)               Not available
.
Other adverse effects       No known significant effects or critical hazards.
SECTION 13	DISPOSAL CONSIDERATIONS	
 Disposal methods          The generation of waste should be avoided or minimized wherever possible. Disposal
                                            of this product, solutions and any by-products should at all times comply with the
                                            requirements of environmental protection and waste disposal legislation and any
                                            regional local authority requirements. Dispose of surplus and non-recyclable products
                                            via a licensed waste disposal contractor. Waste should not be disposed of untreated to
                                            the sewer unless fully compliant with the requirements of all authorities with jurisdiction.
                                            Waste packaging should be recycled. This material and its container must be disposed
                                            of in a safe way. Empty containers or liners may retain some product residues. Avoid
                                            dispersal of spilled material and runoff and contact with soil, waterways, drains and
                                        sewers.
SECTION 14	TRANSPORT INFORMATION	
                                  DOT Classification                   IMDG                                       IATA
UN number                not regulated                         not regulated                         not regulated
UN proper
shipping name                 -----                                      -----                                        -----
transport
Hazard class                     -----                                      -----                                       -----
Environmental
Hazards                             -----                                      -----                                       -----

Special precautions for user:  Transport within user’s premises: always transport in closed containers that are
                                                    upright and secure. Ensure that persons transporting the product know what to do in the
                                                    event of accident or spillage.

Transport in bulk according    Not available.
to Annex II of MARPOL
73/78 and the IBC Code:

SECTION 15	REGULATORY INFORMATION	
U.S. Federal regulations           United States inventory (TSCA 8b): All components are listed or exempted. 
                                                    Clean Water Act (CWA) 307: zinc O,O,O',O'-tetrakis(1,3-dimethylbutyl) bis
                                                   (phosphorodithioate); Zinc alkyl dithiophosphate
                                                    Clean Water Act (CWA) 311: vinyl acetate
                                               This material is classified as an oil under Section 311 of the Clean Water Act (CWA)
                                                    and the Oil Pollution Act of 1990 (OPA). Discharges or spills which produce a visible
                                                    sheen on waters of the United States, their adjoining shorelines, or into conduits leading
                                                    to surface waters must be reported to the EPA's National Response Center at (800)
                                                    424-8802.

Composition/information on ingredients
                                                                              SARA 302 TPQ                     SARA 304 RQ
Name                                                                       %       EHS              (lbs)     (gallons)                     (lbs) (gallons)
Vinyl acetate                                                         <0.01    yes             1000        129                           5000    644.8
SARA 311/312
Classification                        Not applicable.

Composition/information on ingredients

State regulations
Massachusetts                          None of the components are listed.
New York                                   None of the components are listed.
New Jersey                                None of the components are listed.
Pennsylvania                             None of the components are listed.

International regulations          Australia inventory (AICS): All components are listed or exempted.
                                                    China inventory (IECSC): Not determined.
                                                    Japan inventory: Not determined.
                                                    Korea inventory: All components are listed or exempted.
                                                    Malaysia Inventory (EHS Register): Not determined.
                                                    New Zealand Inventory of Chemicals (NZIoC): All components are listed or exempted.
                                                    Philippines inventory (PICCS): All components are listed or exempted. 
                                                    Taiwan inventory (CSNN): Not determined
Canada inventory                      All components are listed or exempted.
EU Inventory                              At least one component is not listed in EINECS but all such components are listed in
                                                    ELINCS.
                                                    Please contact your supplier for information on the inventory status of this material.
WHMIS (Canada)                       Not controlled under WHMIS (Canada).

SECTION 16	OTHER INFORMATION	

National Fire Protection Association (U.S.A.)

 	

	Flammability		
health		Instability/Reactivity		
 		Special		

Reprinted with permission from NFPA 704-2001, Identification of the Hazards of Materials for Emergency
Response Copyright ©1997, National Fire Protection Association, Quincy, MA 02269. This reprinted material is
not the complete and official position of the National Fire Protection Association, on the referenced subject
which is represented only by the standard in its entirety.
Copyright ©2001, National Fire Protection Association, Quincy, MA 02269. This warning system is intended to
be interpreted and applied only by properly trained individuals to identify fire, health and reactivity hazards of
chemicals. The user is referred to certain limited number of chemicals with recommended classifications in
NFPA 49 and NFPA 325, which would be used as a guideline only. Whether the chemicals are classified by NFPA
or not, anyone using the 704 systems to classify chemicals does so at their own risk. 

History
Date of issue/Date of            06/01/2015 
Revision                                                                               
 Key to abbreviations:              ATE = Acute Toxicity Estimate
                                                    BCF = Bioconcentration Factor
                                                    GHS = Globally Harmonized System of Classification and Labelling of Chemicals
                                                    IATA = International Air Transport Association
                                                    IBC = Intermediate Bulk Container
                                                    IMDG = International Maritime Dangerous Goods
                                                    LogPow = logarithm of the octanol/water partition coefficient
                                                    MARPOL 73/78 = International Convention for the Prevention of Pollution From Ships,
                                                    1973 as modified by the Protocol of 1978. ("Marpol" = marine pollution)
                                                    UN = United Nations

THE INFORMATION IN THIS SAFETY DATA SHEET (SDS) WAS OBTAINED FROM SOURCES WHICH WE BELIEVE
ARE RELIABLE. HOWEVER, THE INFORMATION IS PROVIDED WITHOUT ANY WARRANTY, EXPRESSED OR
IMPLIED REGARDING ITS CORRECTNESS OR ACCURACY. SOME INFORMATION PRESENTED AND
CONCLUSIONS DRAWN HEREIN ARE FROM SOURCES OTHER THAN DIRECT TEST DATA ON THE SUBSTANCE
ITSELF. THIS SDS WAS PREPARED AND IS TO BE USED ONLY FOR THIS PRODUCT. IF THE PRODUCT IS USED
AS A COMPONENT IN ANOTHER PRODUCT, THIS SDS INFORMATION MAY NOT BE APPLICABLE. USERS
SHOULD MAKE THEIR OWN INVESTIGATIONS TO DETERMINE THE SUITABILITY OF THE INFORMATION OR
PRODUCTS FOR THEIR PARTICULAR PURPOSE OR APPLICATION.
THE CONDITIONS OR METHODS OF HANDLING, STORAGE, USE, AND/OR DISPOSAL OF THE PRODUCT ARE
BEYOND OUR CONTROL AND MAY BE BEYOND OUR KNOWLEDGE. FOR THIS AND OTHER REASONS, WE DO
NOT ASSUME RESPONSIBILITY AND EXPRESSLY DISCLAIM LIABILITY FOR ANY LOSS, DAMAGE OR EXPENSE
ARISING OUT OF OR IN ANY WAY CONNECTED WITH HANDLING, STORAGE, USE OR DISPOSAL OF THE
PRODUCT.